BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1709
Answer signal ?

The command is used to state whether the line signal “answer” shall be sent at an incoming call when the call is answered in the exchange.

Note

Ascertain that the signal is included in the selected line signal scheme.

Value: YES or NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003