BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8713
Automated Attendant error reroute positon

In selections list it is possible to program an exit position (for time-out and cases of wrong entries).

In this command you must specify the directory number of the exit position.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003