BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8104
Paging absence ?

This command is used to determine whether the absence signal shall be used or not.

In certain cases the paging equipment can send an absence signal to the exchange in order to state that e.g. the paging receiver is in its charging shelf. In such case the pager receives the absence message.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003