BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2110
Delay voice announcement

An external call directed to a facility with automatic answer, in form of a voice announcement, will be answered after a programmable delay time. During the waiting, the external party will hear ring tone.

This command defines the delay time. The programmable time is the minimum delay time for an external call when the call is automaticaly answered with a voice announcement. The delay time is programmable from 0 to 30 seconds. Default value shall be 0, no delay is programmed.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003