BusinessPhone Communication Platform 4.0
Dialogs

## Virtual Private Network From PSTN

To access the dialog, open the “System” menu in the Configuration directory tree. Next open the “System facilities” submenu and click on “VPN from PSTN”.

The following commands are available:

2090 |  | VPN Service from PSTN

2091 |  | Predigits sent to PSTN-VPN

2092 |  | Trunk route selected as PSTN-VPN call

#### Actions

Submit |  | To send your changes to the system. |
Reload |  | To discard any changes and to reload the user data. |

See facility description Networking – VPN Service From PSTN (364/15534-ASB 150 02 Uen).

Revision: A © Ericsson Enterprise 2003