BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4012
Sending a ready tone after announcement

The command defines whether a toneburst (TONE.OKAY) shall be sent to the operator after sending of the individual operator announcement has been completed.

Alternatives:

YES = |  | A tone burst will be sent to the respective operator after the individual operator announcement has been send.

NO = |  | No tone burst will be sent to the respective operator after the individual operator announcement has been sent.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003