BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8902
CTI route timeout

This command is used to set the time during which the PBX waits for an automatic reroute position from a CTI telephony server. Valid settings for this parameter are from 1 to 30 seconds. The default value is 4 seconds.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003