BusinessPhone Communication Platform 4.0
Commands > Commands 7000...7999

## 7506
High traffic limit timer

Indicates the minimum number of free timers that must exist in the system, so that new calls from extensions will not receive congestion tone when attempting a call. Value 0-250 free timers.

The limit is there to ensure, at peak periods, that there will be enough CPU-resources for the traffic already ongoing in the exchange.

See also command 7507 Max traffic limit timer.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003