BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0112
Destination of fixed diversion

The command states the diversion address, i.e. the predetermined divertee position to which incoming calls to the extension are to be diverted.

The divertee position is specified by stating the directory number of the divertee position.

For this command the directory number is not checked. However diversion will be executed only if the directory number is one of the following:

- extension number
- PBX-operator number
- extension (PBX) group number
- voice answer number
- voice message number
- fictive number
- standard paging number
- common short number
- automated attendant number
- private network number

The divertee position is erased by overwriting the directory number with blanks.

For diversion to take place, at least one of the facilities direct diversion, diversion on no-reply, or diversion on busy must be activated.

The divertee position can also be altered by extension users themselves via individual programming.

Valid data: 1 - 8 digit directory number

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003