BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1608
Call meter receiver level

The command is used to state the detection level for the charging pulse tone receivers CM 12/16, ROA 219 5062/1 and CM 12, ROA 219 5062/2.

The type of the pulse tone receiver (12 kHz or 16 kHz) is defined by command 1607 Call meter type.

Two trunk individuals using the same daughter board, CM 12/16 or CM 12 shall be programmed with the same values for command 1607 Call meter type and 1608 Call meter receiver level.

Detection level for pulse tone receivers CM 12/16 (with CML circuit), ROA 219 5135/1 is defined by command 1614 Call meter (CML) receiver level.

Charging with 50 Hz is not affected by this command.

Value: Corresponding detection level:

CM 12 | CM 12/16
12 kHz | 12 kHz | 16 kHz
(0) | -19.0 dBu | -21.5 dBu | -19.5 dBu
(1) | -20.0 dBu | -25.0 dBu | -23.0 dBu
(2) | -22.0 dBu | -27.0 dBu | -25.0 dBu
(3) | -24.0 dBu | -31.0 dBu | -29.0 dBu
(4) | -26.0 dBu | -33.0 dBu | -30.5 dBu
(5) | -28.0 dBu | -35.0 dBu | -32.5 dBu
(6) | -30.0 dBu | -38.0 dBu | -36.0 dBu
(7) | -33.0 dBu | -43.0 dBu | -40.5 dBu

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003