BusinessPhone Communication Platform 4.0
Dialogs

## Board Configuration

Note

This feature is only available for BusinessPhone V5.0 (ASB 150 02 R12) or later versions!

In this dialog, you can view the number of licensed voice channels, set the number of trunk individuals and IP extension, and define a IP extension threshold.

To access the Board Configuration dialog, open the “System” menu in the Configuration directory tree. Then open the “System parameters” submenu and click on “IPU board data...”. On top of the dialog, you find a navigation bar. Click on “Board configuration” to open the dialog.

Note

The number of available voice channels depends on the license, and the sum of trunks and the extension threshold may not exceed the number of voice channels!

### Other IPU Board Data dialogs

On top of the dialog, you find a navigation bar that provides access to the following IPU Board Data dialogs:

- Basic Data

- To open the Basic IPU Data dialog.

- Network IP address

- To go to the Network IP address dialog.

- Ports

- To go to the Port configuration data dialog.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |
Board Info |  | To view the Board Information dialog. |

Revision: A © Ericsson Enterprise 2003