BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9123
Predigits choice 2

This command is used to define predigits, if any, for the 2-nd route choice. The predigits are transmitted after the private network access code and before the dialled external number.

Predigits = 1-16.

Following commands for the 2-nd route choice will be ignored:

3302 |  | Call back allowed

3303 |  | Predigits

3304 |  | Alternative route choice 1

3305 |  | Predigits choice 1

3306 |  | Alternative route choice 2

3307 |  | Predigits choice 2

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003