BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8203
Receiver type

This command is used to determine the type of paging receiver.

0 = |  | “Bleeper” type receiver without display

1 = |  | Display receiver for call-me paging

2 = |  | Receiver with speech option without display

3 = |  | Receiver with speech option with display

4 = |  | Group call without display

5 = |  | Group call with display

6 = |  | Display receiver for meet-me paging

For standard paging the receiver type is used to determine the type of paging to be started.

For alternative paging, a check takes place to verify that the requested paging can be handled by the receiver.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003