BusinessPhone Communication Platform 4.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 52 MEMEX

0 RPM_NAK |  | Subcode not implemented |
1 RPMREAD |  | Read in RP memory |
2 RPMREAD_ACK |  | Answer on RPMREAD |
3 RPMREAD_NAK |  | Answer on RPMREAD |
4 RPMWRITE |  | Write in RP memory |
5 RPMWRITE_ACK |  | Answer on RPMREAD |
6 RPMWRITE_NAK |  | Answer on RPMREAD |

Revision: PD2 © Ericsson Enterprise 2003