BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x84
No IND-DATA Received On Request

Default definition: |  | ERROR + TRIG |
Used by block: |  | EX |
Category: |  | DESIGNER |

An INDDATAREQ message was answered with an empty INDDATAANSW message. Normally the INDDATAREQ/INDDATAANSW sequence is used in the display handler, when the display should be updated.

- D1: Current LCD-state.
- D2: Current process state.
- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003