BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8703
Digit 0 related dir no

According to the current structure of Automated Attendant-network, you can specify the addressing of these commands. The addresses can be:

- directory numbers of physical extensions, or
- directory numbers of another AA or
- operator queue, ACD queue or PBX group
- common abbreviated numbers or
- directory number of a common or individual mailbox or DISA directory number

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003