BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8105
Paging channel

The paging equipment is connected to ASB150 via one or more trunks, depending on how many channels are desired.

If several channels shall exist, these trunks must be placed in one route.

This command is used to determine the channel number, i.e. the call number of the paging equipment. The number shall be either the directory number of the trunk or route, depending on whether one or several channels shall exist.

The stated channel number must exist in the system.

When paging is initiated, paging code, mode digit/message (if used) are sent to the paging equipment via the paging channel stated in this command.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003