BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1943
UU-information in ALERT message

This command states whether or not it is allowed to include UUI (User-to-User Information) in the ALERTING message at this interface.

Valid data:

No |  | not allowed

Yes |  | allowed

DMinimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003