BusinessPhone Communication Platform 4.0
Dialogs

## Hardware survey

This dialog gives an overview about the boards that are located in each cabinet.

To access the dialog, click on the “Boards” menu in the Configuration directory tree. The context menu appears. Select “Hardware survey” from the context menu to open the dialog.

### Adding or changing a board - offline

- To add a new board, click on the “...” button of an empty field in one of the cabinets. To change a board position, click on the “...” button of the respective board.
- The Hardware survey – Card Selection dialog opens. The cabinet and board position that have been selected in the previous dialog are displayed on top of the window. If you have selected a vacant position, the radio button “empty” is marked. If you want to change an existing board position, the respective board type radio button is selected automatically.

Note

You cannot change the cabinet and board position in this dialog. To move boards go to Swap boards.

- Select a card type by clicking in the respective radio button and click on OK.

- Or:

- Click on Cancel to abort the process and to return to the previous dialog without any changes.
- Click on Submit to send your changes to the system. The dialog refreshes, now showing the new board resp. the changed board information in the selected position.

Note

Non-self reporting cards are not available OFFLINE; non self reporting cards can be added ONLINE only.

#### Actions - offline

Submit |  | To submit your changes to the system. |
Swap boards |  | To show Swap boards |
Details |  | To show Hardware Details |

### Adding or changing a board - online

- Only the following non self reporting boards can be added or changed in this dialog:

- AUX3 (ROF 157 5119/3)
- TBU (ROF 157 5126/2)
- IC-LU (ROF 157 5129/1)
- Integrated battery unit (BKB 201 001)
- RESERVED

- To add a new non self reporting board, select a offered position (not occupied by a self reporting board) and choose the desired board.
- The article number has to be entered manually (e.g. ROF 157 xxx)
- Click Set to send your changes to the system. The dialog refreshes, now showing the new board in the selected position.
- The settings can be stored in ASB 150 02 by the standard backup function of BMS.

Note

A transfer after cold-start does not transfer the non self reporting boards.

For more information, see section Hardware survey – Card Selection and Installation Instruction ASB 150 02 (1531-ASB 150 02 Uen).

#### Actions - online

Set |  | To send your changes to the system. |
Details |  | To show Hardware Details |

Revision: A © Ericsson Enterprise 2003