BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6103
Set hour minute second

Enter time:

Format: HHMMSS

Minimum required authority level from telephone: 1

Accessible via BMS: No (It is possible to programm this command also via RASC but only in the application "MAINTENANCE" and it is not possible to find this command with the search function "F3".)

Revision: A © Ericsson Enterprise 2003