BusinessPhone Communication Platform 4.0
Warning Messages ASB 150 02 >

## 0x72
Invalid Parameter At Startup

Default definition: |  | ERROR |
Used by block: |  | SU |
Category: |  | DESIGNER |

An invalid parameter value has been found by SU. The meaning of D1 depends on the value of D2.

D2 | Type of error | D1 | Additionl data
00h | Not defined |  |
01h | Default data length error for the E2BASE |  | Block ID (ST)
02h | Card table access error |  | Given card position
03h | ID error on answer from the E2-handler |  | Received card position
04h | Highest reported individual |  | Reporting card position number too high
05h | The data length for the individual RAM record in the REPORT table is higher than 125 bytes |  | Individual type

- D3: Undefined
- D4: Undefined

Revision: F © Ericsson Enterprise 2003