BusinessPhone Communication Platform 4.0
Commands > Commands 7000...7999

## 7437
Max active alarms per day

This command determines the maximum number of active alarms that may be sent every day to an external alarm receiver (alarm centre). Value 0-255 a day.

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003