BusinessPhone Communication Platform 4.0
Installation Instruction ASB 150 02

## Installation Of FILTER BOX (BDV 113 31) With BE12/16, Call Metering Filter Board (ROA 219 5110/1, -/2), Mounted

Mount the FILTER BOX (BDV 113 31) on the wall, just as the MDF under External MDF SXK 106 4139/1.

Installation of BE12/16 is to be made as shown in the figure below.

If surge protectors are installed, the FILTER BOX must be connected to earth.

Revision: A © Ericsson Enterprise 2003