BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0143
Line break for ELU-A

Line break for analog extension.

With this command you can state the duration of a line break for an analog extension.

Valid values for this command are 0-255.

The value zero indicates no line break.

The duration of a linebreak can vary from 1 * 50 ms to 255 * 50 ms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003