BusinessPhone Communication Platform 4.0
Fault Tracing ASB 150 02 > Fault locating

## Flow Charts for Cordless

#### Flow Charts for Cordless – Part 1

#### Flow Charts for Cordless – Part 2, Common User complaint

#### Flow Charts for Cordless – Part 3, Individual User complaint

#### Flow Charts for Cordless – Part 4, Errors

#### Flow Charts for Cordless – Part 5, No Dial Tone

#### Flow Charts for Cordless – Part 6, CSM Problem

#### Flow Charts for Cordless – Part 7

### Completion of service

On completion of service disconnect RASC and check the warning log for entries. If this is the case adopt the recommended measure(s). If no further measures can be taken note the logs (or printout if possible) and contact your local support facility.

Remaining faults are to be reported (see Fault reporting).

If you cannot fix the problem at the moment start up the exchange again and give the customer instructions how to cope with malfunctions, conclude by making a printout of the warning log and resetting it. Disconnect RASC and place the cover on the exchange.

Revision: F © Ericsson Enterprise 2003