BusinessPhone Communication Platform 4.0
Dialogs

## Board Information

The Board Information dialog is a read-only dialog showing the hardware information of a certain board. It is also possible to shut down or activate a board remotely. Please note that the sections Article Information and FECU Information are only available for online system connections.

Column | Description
Name | Shows the name of the selected board
Cabinet | States the cabinet in which the board is mounted
Position | States the position of the board
R-state PCB | States the revision of the unassembled printed circuit board
HW-Code | States the revision of the assembling of the printed circuit board
ROF Info | Sates the article number of the board

### Groups on board

- Individual TYPE of the board
- # shows the number of individuals of this type
- V. (Version) of individual type 0-15. The version number is used to give some additional information of the installed devices.

TYPE | V. | NOTE
ELUD | 0 | For DBC-6xx, 2xx, 1xx instruments (at ELU-D)
ELUD | 1 | For IP clients (located at IPU)
ELUA | 0 | Analogue instruments (at ELU-A)
ELUC | 0 | For DBC-7xx instruments (at ELU-C)
ICCU | 0 | CORDLESS equipment (A protocol)
ICCU | 1 | CORDLESS equipment (GAP protocol)
IOU | 0 | V-24 and 50 Hz, 24 receivers (at CMU)
IOU | 1 | V-24 and 12/16 kHz, 8 receivers (at CMU)
IOU | 2 | (reserved for CMU)
IOU | 3 | V-24 (located at CPU-D or AUX)
IOU | 4 | V-24 (located at IPU)
SMU | 0 | V-23 modem (located at CPU-D)
RSU | 0 | Register (located at BTU-D for CAS)
RSU | 1 | Register (located at BTU-D for ISDN)
RSU | 2 | Register (located at VMU-HD)
RSU | 3 | Register (located at MFU)
VMU | 0 | Voice memory (VMU-D).
VMU | 1 | Voice memory (VMU-HD).
BTUDC | 0 | CAS-trunk (at BTU-D)
BTUA | 0 | Analogue trunk (BTU-A)
BTUA | 1 | Analogue trunk DC-Loop (BTU-C, trunk line)
BTUA | 2 | Analogue trunk E&M (BTU-E)
BTUA | 3 | Analogue trunk DC-Loop (BTU-C, tie line)
BTUDP | 0 | ISDN-trunk, primary access (at BTU-D) *)
BTUB | 0 | ISDN-trunk, basic access, T-interface
BTUB | 1 | ISDN-trunk, basic access, S-interface
BTUB | 2 | ISDN-trunk, basic access, IP-interface
- | - | Spare for future
- | - | Spare for future
IPU | 0 | This type is used to identify the common IP data (non-individual). It must not be used for reporting.
TSU | 0 | Tone sender, located at CPU-D TYPE.TSU must be reported first by the RP at CPU-D, this individual type is used to identify the whole CPU-D card.

For more information on boards, see Installation Instruction ASB 150 02 (1531-ASB 150 02 Uen), and document Maintenance Instruction(1541-ASB 150 02 Uen).

### Shutting down a board

The shut down command must be executed before removing one or more board(s), in order to avoid a system restart.

Note

To shut down a board, the board must be registered in the E2 memory of the CPU-D4. You cannot shut down a misplaced or missing board or a wrong type of board.
Before shutting down an IC-CU_ board, it is recommended to save the data using the DECT Backup System (CSM) or the BMS (only IC-CU2). After replacing the IC-CU_ board, the configuration data from the previously installed board has to be uploaded again, otherwise you have to re-program all cordless telephone sets.

- Click on the Shut down button to deactivate the board

- If the shut down should not be performed immediately, enter a time frame between 0 and 11 minutes. After this time has expired, all active processes on the board will be terminated.

### Replacing a board

- After you have shut down a board, wait until the new status is displayed.
- Replace the board by a new board of the same type.
- Click on the Activate button to activate the board.

When the process has been completed, a confirmation is displayed, containing all the data of the operational board (PROM version, revision, etc.).

#### Actions

Restart |  | To restart the selected board. |
Delay |  | Minutes left till the restart will be performed. Select a number from the drop-down list. |
Shutdown |  | To shutdown a specific board. |
Voice Channel Licensing |  | To view the Voice Channel Licensing dialog and to read out details about the IPU licensing. Note This button is only available if the IPU application image RYS 102 541/1 ³ R2A is used. |
Board configuration |  | To go to the Board Configuration dialog. |

Revision: A © Ericsson Enterprise 2003