BusinessPhone Communication Platform 4.0
Installation Instruction ASB 150 02

## Marking Of Cables

Each cable that is connected to a PBX type ASB 150 should be marked on the cable’s designation holder with the label set SVH 277 003/4, supplied for this purpose. The cable TSR 902 0444/1 is supplied with a designation holder, 860 1839, at the EURO-connector.

This label set contains three label types:

Label 1: |  | This label indicates the abbreviated name for the PBA to which the cable is to be connected. Example of parameter:

Label 2: |  | There is one 2-digit parameter. This parameter indicates the position of the PBA-slot in the PBA where the cable is to be connected. Example of parameter:

Label 3: |  | There are two 1-digit parameters. The first parameter indicates the position of the pin-contact unit on the PBA. The second parameter indicates the 1/4 of the pin contact. Example of parameters:

These three labels indicate where the upper part of the cable is to be connected and are placed on the front side of the designation holder.

When the label 1 for PBA has a "_" included in the name, please enter the correct letter with a marker pen.

### External MDF SXK 106 4139/1

1. Unpack the MDF cabinet and remove its front cover.
2. Mount the MDF cabinet on its designated position. Take into consideration the normal working height above the floor (about 1.30 m to the lower edge of the MDF cabinet) and the length (1.5 m) of prefabricated cable TSR 902 0444/1.

- Overall dimensions of the MDF cabinet: 295x184x68 (HxWxD in mm).

1. Loosen cover only by hand force (there are no holding screws)
2. Mark mounting holes for MDF cabinet
3. Drill and insert plugs (Use enclosed screws and plugs)
4. Mount MDF cabinet and screw it securely into position

Revision: A © Ericsson Enterprise 2003