BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6303
Log minimum meter pulses

This command can be used if it is desired to log outgoing external calls (see command 6301 Log outgoing calls?), but exclude those calls that have incurred “few” meter pulses.

The command is used to determine the minimum number of meter pulses required for an outgoing external call to be logged.

Value = 0-9999 meter pulses

Further prerequisites can be defined for determining which outgoing external calls shall be logged, see commands 6302 Log duration time and 6306 Log dialled numbers beginning with 0-6315 Log dialled numbers beginning with 9.

With the minimum number of meter pulses = 0000, outgoing external calls will be logged irrespective of the number of meter pulses.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003