BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6720
Operator password

This command states the password for the superuser. With function code * 45 # and this password, you have access to the costs of other callers and trunk lines.

Value: 1-10 digits (0-9), *, #, mute and status

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003