BusinessPhone Communication Platform 4.0
Fault Tracing ASB 150 02 > Procedures

## Check RASC connection

When encountering communication failures to RASC verify proper settings for the V.24-port and the programmable parameters for the built-in modem and corresponding parameters for RASC on the PC. For more information consult document EN/LZB BS 103 1197 RASC Uen, "RASC".

Revision: F © Ericsson Enterprise 2003