BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1942
UU-information length for UUS service 1

This command states which maximal UUI (User-to-User Information) length in UUS (User-toUser Signalling) service 1 is supported at this interface.

Valid data:

0 |  | 128 octets

1 |  | 32 octets

DMinimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003