BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2008
Verification tone on call back

The system supplies normal verification tone when it accepts an order. This can be altered so that silence is received instead.

Valid data: |  | YES (verification tone)

|  | NO (silence)

Default data: |  | YES

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003