BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4011
Listening during the announcement

The command defines whether the operator can listen into the incoming trunk line while the individual operator announcement is played. By default the operator hears nothing at all. A tone burst and arrows on the display indicate that speech connection is established after the announcement has been played.

Alternatives:

NO = |  | Listening into the line while operator announcement is switched off.

YES = |  | Listening into the line while operator announcement is switched on.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003