BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1402
Time supervision of long register sign. alt. MFC/MFE outgoing

The command is used to determine the time for long supervision before the first digit and between the digits when dialing. Value 3-255 seconds.

Timeout results in disconnection/blocking, unless an open number has been received from the TCD-analysis, or a switch to speech state if an open number has been dialed.

Note

For decadic pulsing this time must not be less than the time required by the BTU-board to transmit the digit.

(See commands 1401 Number of digits with long dial supervision and 1403 Time supervision of short register sign. alt. MFC/MFE outgoing = the relationship between the number of digits and the time for supervision is adapted for possible standard number series for the line.)

For ISDN ( BTUDP, BTUB ) trunks the command is valid only in case of MLT-system configuration.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003