BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4310
Keep answered voice

This command states how many answered voice messages can be saved. Thus the size of the part of the E2 memory to be used for answered messages can be determined.. This, of course, reduces the space for unanswered messages correspondingly.

Value 0 means that an unanswered message will be erased automatically upon answer except in case of a display telephone, where the message is erased by means of a command. The range of values 1-99 specifies the number of answered messages saved. They can be accessed by means of a special procedure.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003