BusinessPhone Communication Platform 4.0
Dialogs

## System Data

Generates the required system data for your BusinessPhone system.

To access the dialog, open the “System” menu in the Configuration directory tree and click on “General”.

The dialog comprises the following sections:

- Ring and Tone Signals
- Text Mode
- Analogue Extension Parameters
- Digital Extension Parameters
- Cordless Extension Parameters
- Miscellaneous

On top of the dialog, you find a navigation bar for direct access to each of the sections.

See System Overview (1555-ASB 150 02 Uen).

### Ring and Tone Signals

#### General

2001 |  | Ring signal scheme

2093 |  | Conversation recording tone

#### Outgoing calls

2008 |  | Verification tone on call back

2027 |  | Length of inactivity

2028 |  | Ringtime for internal calls

2030 |  | Disconnection tone for digital extensions

#### Incoming calls

2029 |  | Repetitive call-waiting tone

### Text Mode

2070 |  | Keypad characters

- Characters for keys 0 to 9 and the star key.

#### National keys

2003 |  | National key (Inquiry)

2004 |  | National key (Hold)

2005 |  | National key (Read&)

2006 |  | National key (Transfer)

See facility description Text Mode (483/15534-ASB 150 02 Uen).

### Analogue Extension Parameters

2007 |  | Rotary dial type

2025 |  | Nominal impedance for analogue extensions

2026 |  | Attenuation for DTMF-signalling

### Digital Extension Parameters

#### Loudness rating

2032 |  | Sidetone masking rating

2033 |  | Sending Loudness Rating

### Cordless Extension Parameters

#### GAP parameters

2094 |  | GAP Version

### Miscellaneous

#### Services

2036 |  | Call pickup of reminder/call back allowed

2056 |  | Shut down reroute position

2080 |  | Free second access

2081 |  | Modified business key layout

2082 |  | Transfer via hookon

#### PCM Channels

2011 |  | PCM-channels reserved for external lines

#### Voice Mailbox

2023 |  | External voice mail directory number

See facility description Mailbox system (340/15534-ASB 150 02 Uen).

#### Traffic Limits

7506 |  | High traffic limit timer

7507 |  | Max traffic limit timer

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See facility description Analogue Telephone (111/15534-ASB 150 02 Uen).

Revision: A © Ericsson Enterprise 2003