BusinessPhone Communication Platform 4.0
Commands > Commands 4000...4999

## 4007
Queue announcement reference

A voice message can be supplied to external incoming calls in the PBX-operator queue. This command is used to state the reference number for a voice message.

The reference number is entered as: uuvv

where

uu = |  | 01 (always)

vv = |  | 01-32 (see command 4401 Voice Announcements)

uuvv = |  | blank (no voice message)

It is required that the stated reference (uuvv) has been recorded with a system telephone in accordance with command 4401 Voice Announcements.

The duration of the voice message shall be stated with command 4006 Queue announcement time.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003