BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2024
Initiate public Dialtone at LCR

This command is used to state whether the public dialtone has to be sent to the caller, after dialling a directory number of a LCR-controlled trunk. The parameter programmed by this command is relevant only if command 2034 Initiate dial tone at LCR is set to YES. See command 1028 LCR analysis required ?.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003