BusinessPhone Communication Platform 4.0
Commands > Commands 8000...8999

## 8202
Search Code

When paging is to start, a paging code is sent to the paging equipment. The paging code is the paging receiver’s identity in the paging equipment.

This command is used to determine the paging code to be sent to the paging equipment on a call to a receiver.

Paging to a certain receiver can be prevented by erasing the paging code.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003