BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1012
Reroute on answering position busy ?

The command is used for in-dialing and for private lines to reroute incoming calls to the rerouting position, if the required destination is marked busy.

For rerouting to take place, the rerouting position must have been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003