BusinessPhone Communication Platform 4.0
Commands > Commands 7000...7999

## 7432
Active alarm receiver

This command determines the signalling method to be used when sending active alarms.

Different types of alarm receivers (alarm centres) often use different signalling methods.

For a description of the different signalling methods provided, see command 6006 Device type.

‘Active alarm’ is a function which transfers alarms to an external alarm receiver.

Commands 7420 Service area id, 7421 Identity of exchange and 7430 Active alarm on?-7437 Max active alarms per day concern active alarms.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003