BusinessPhone Communication Platform 4.0
Facilities

## Fault Indication

## Definition

Fault indication enables the signalling of a fault as selected in the RASC tables, on a digital system telephone set with display.

## Use

This function can be used when certain alarms detected by the system should be signalled on a digital system telephone set.

## Operation

### STANDARD-, EXECUTIVE Telephone and OPERATOR Console

There are a number of alarms that are detected by the system which can be indicated on a digital telephone set (e.g. LED lights on function key).

When the programmed function key indicates an alarm, press the key and the alarm code is displayed on the display.

Press “Enter” to clear this display and step to the next masked alarms.

## Capacity

This feature can be activated on all digital system telephone sets with programmable function keys.

## Limitations

Not available on analog telephones and on digital telephone sets without programmable function keys.

## Programming

### The following commands are only accessable via BMS/RASC:

To flag the warnings that are to be indicated, enter under Maintenance/logging and select from defined codes for example:

0302 |  | Number/ID

Insert the code *91# on selected key to display all flagged alarms.

## Equipment

None

Revision: B © Ericsson Enterprise 2003