BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2501
Programming of abbreviated numbers

Each common abbreviated number is programmed in an abbreviated number table.

- Enter directory number for abbreviated number
- Enter relevant abbreviated number.
  maximum 23 digits (1-9, 0, *, #).

Default data = No number

Wait for intermediate tone by pressing the “-”-key via BMS / RASC.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003