BusinessPhone Communication Platform 4.0
Commands > Commands 5000...5999

## 5902
Line position-directory number

With this command it is possible to read information about a line position in the exchange.

The line position is specified as circuit board position and individual number on this board.

The displayed information concerns an individual on the board that has been made operational at this position, even if this board has not been mounted.

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003