BusinessPhone Communication Platform 4.0
Commands > Commands 1000...1999

## 1708
EOS-signal ?

The command is used to state whether the line signal “End-Of-Selection” (EOS) shall be sent after the full number has been received at an incoming call.

Note

Ascertain that the signal is included in the selected line signal scheme.

Value: YES or NO

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003