BusinessPhone Communication Platform 4.0
Commands > Commands 9000...9999

## 9113
Predigits choice 1

This command is used to define predigits, if any, for the first route choice. The predigits are transmitted after the private network access code and before the dialled external number.

Predigits = 1-16.

Following commands for the 1-st route choice will be ignored:

3302 |  | Call back allowed

3303 |  | Predigits

3304 |  | Alternative route choice 1

3305 |  | Predigits choice 1

3306 |  | Alternative route choice 2

3307 |  | Predigits choice 2

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003