BusinessPhone Communication Platform 4.0
Commands > Commands 6000...6999

## 6006
Device type

The command defines to which type of connected unit the I/O-port is to be adapted.

The used line protocol (if any) is described in document 1/15519 ASB 150 01 Uen, “Interwork Description”.

In some cases, master/slave must also be stated by means of command 6010 Master/Slave. When programming the unit, the values of several parameters adapted for the connected unit will be set automatically. (See tables below).

Unit values:

0 = |  | Unspecified terminal

1 = |  | Operation and maintenance centre (O&M) with ECOM/ECEL

2 = |  | Unspecified printer/terminal

3 = |  | Printer type 1 (e.g. FACIT 4510)

4 = |  | Printer type 2 (e.g. ERICSSON 7111)

5 = |  | Computer for administration of call information logging (CIL)

6 = |  | Computer for administration of call information logging (CIL)

7= |  | Unspecified printer/terminal

8 = |  | Connection to computer with standard hotel line protocol. The PABX is master, the hotel computer is slave

9 = |  | Connection to computer with standard hotel line protocol. The PABX is master, the hotel computer is slave

10 = |  | Connection to computer with line protocol type 3

11 = |  | Operation and maintenance centre (O&M centre) with RASC and MS

12 = |  | Connection to computer with line protocol type 2

13 = |  | Hotel computer, bi-directional V.24 interface with line protocol type 4

14 = |  | ASB15002 test protocol

15 = |  | Common O&M interface for CSM

The following parameters are assigned values:

Administration of circuit 105-109 in the V.24 interface |  | 105-109 |
Parity check |  | Pcheck |
Echo |  | Echo |
Number of stop bits |  | Sbits |
Word length |  | Wlength |
Line protocol |  | Protocol |
Set of check characters |  | Sochar |

Unit |  | 105 - 109 |  | Pcheck |  | Echo |  | Sbits |  | Wlengh |  | Protocol |  | Sochar |
0 |  |  |  |  |  |  |  | 1 |  | 8 |  | **0 |  | *1 |
1 |  |  |  |  |  |  |  | 1 |  | 8 |  | **1 |  | *2 |
2 |  |  |  |  |  |  |  | 2 |  | 7 |  | **0 |  | *3 |
3 |  |  |  |  |  |  |  | 1 |  | 8 |  | **2 |  | *4 |
4 |  |  |  |  |  |  |  | 1 |  | 8 |  | **2 |  | *5 |
5 |  | Yes |  | Even |  |  |  | 1 |  | 7 |  | **0 |  | *1 |
6 |  | Yes |  | Even |  |  |  | 1 |  | 7 |  | **3 |  | *2 |
7 |  |  |  |  |  |  |  | 1 |  | 8 |  | **2 |  | *3 |
8 |  |  |  | Even |  |  |  | 1 |  | 7 |  | **4 |  | *2 |
9 |  |  |  | Even |  |  |  | 1 |  | 7 |  | **4 |  | *2 |
10 |  |  |  |  |  |  |  | 1 |  | 8 |  | **5 |  | *2 |
11 |  |  |  |  |  |  |  | 1 |  | 8 |  | **6 |  | *2 |
12 |  |  |  | Even |  |  |  | 1 |  | 8 |  | **4 |  | *2 |
13 |  |  |  | Even |  |  |  | 1 |  | 8 |  | **7 |  | *2 |
14 |  |  |  |  |  |  |  | 1 |  | 8 |  | **8 |  | - |
15 |  |  |  |  |  |  |  | 1 |  | 8 |  | **9 |  | *2 |

Protocols:
**0) |  | Standard without flow control |
**1) |  | PABX's remote transmission protocol |
**2) |  | Standard with flow control (X-on/X-off) |
**3) |  | Computer communication TYPE 1 |
**4) |  | Computer communication TYPE 2 |
**5) |  | Computer communication TYPE 3 |
**6) |  | ASB 150 long-distance communications protocol for multichannel function |
**7) |  | Computer communication type 4 |
**8) |  | PC-Operator V1.x and testtools |
**9) |  | Cordless System Manager (CSM) |

Check characters:
*1) |  | PABX's internal, without conversion |  |  |
*2) |  | According to line protocol |  |  |
*3) |  | Simple standard |  |  |
*4) |  | Subset of PABX's internal |  |  |
*5) |  | New line: |  | CR |
|  | New page: |  | FF |
|  | Bold print: |  | ESC E |
|  | Underlining: |  | ESC-1 |
|  | Elongated print: |  | ESC W 1 |
|  | Reset: |  | ESC F ESC-0 ESC W0 |

Note

If set to value 14 (ASB15002 Test Protocol) AND command 6431 Test protocol port address is set to current port, this value can no be changed unless 6431 is reprogrammed!

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003