BusinessPhone Communication Platform 4.0
Commands > Commands 0000...0999

## 0110
Diversion on no reply at internal calls ?

The command defines if a diversion on no-reply on an internal call should be done.

If the extension is a master and member of a tandem configuration the command data shall be copied to the slave and blocked for the slave's further use.

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003