BusinessPhone Communication Platform 4.0
Fault Tracing ASB 150 02 > Procedures

## Check CSM connection

The Cordless System Manager software installed on a PC requires a connection to the maintenance port on the Cordless System Central Unit (IC-CU_) or to the CPU-D4, either to the maintenance port or via modem. Off-line menus include functions that do not require this connection. Go to the directory in which the Cordless System software has been installed9ply started-up the welcome menu is displayed.

If there is no communication with the Cordless System the message ’No connection with DCT1800. Start Off-line program? Y (Yes/No)’ is displayed. By pressing the <Enter> key the Off-line program is started. If you want the connection with the Cordless System you must now check the connection between the PC and the Cordless System and then select N(o). If communication has not been established yet, the following message ’Waiting for DCT1800 response...’ is displayed. If there is still no communication with the DCT1800 system the message ’No connection with DCT1800. Do you wish to continue? (Yes/No)’ is displayed.

When the communication is established the message ’Loading data from DCT1800, please wait...’ is displayed.

If the Cordless System has been initialized before with a version of the Cordless System Manager older than revision R6, the message ’WARNING: SPU-S parameters not initialized yet. <Enter>’ is displayed. If so, do not forget to execute the ’Restore country data’ command.

Revision: F © Ericsson Enterprise 2003