BusinessPhone Communication Platform 4.0
Commands > Commands 2000...2999

## 2503
Abbreviated number category 1

This command defines whether or not the abbreviated number shall be available for the abbreviated number category 1.

Y = |  | Open for category

N = |  | Blocked for category (default data)

An existing abbreviated number is erased by pressing the “-” -key on the phone. This key can also be used as backspace during programming of an abbreviated number.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: A © Ericsson Enterprise 2003